## **IKEA Package Test Application Form** QF 701-2N

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Applicant Information** | Supplier No: | Supplier Name: | | | |
| Supplier Address: | | | | |
| Supplier Contact: | | Phone/Mobile: | | E-mail: |
| IKEA Contact: | | E-mail: | | |
| **Invoice Information** | Invoice Title : | | | | |
| Invoice delivery address: | | | | |
| Invoice Contact: | | Phone/Mobile: | | E-mail: |
| VAT no: | | | | |
| Service required: Regular Express | | | |  | |
| Product Testing Types: Verifying Test\* Prototype Test  \*By signing Verifying test, the supplier accepts that the results and the test report are shared with concerned co-workers at Inter IKEA. | | | | | |

**Sample Information** (Items with \* are very important. Without \*Paper Composition; \*Batch number / Product date, you run the risk that TR not complying with all IKEA requirements for the required information)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Article** | | | | | |
| Article No. : | | Article Name | | | Date Stamp/Production Date: |
| **Raw Material** | | | | | |
| ***Basic information:*** | *\*Material Producer:* | | | *Material Description:* | |
|  | *\* Batch Number / Production Date:* | | | *Sample Amount:* | |
| ***Corrugated Board:*** | *\*IKEA CB Code:* | | *\*CB Colour:* *Brown/Brown, White/Brown, White/White* | | |
|  | *\*Flute Type:* *E,* *B,* *C,* *A,* *BA,* *BC, AC, Other:* | | | | |
|  | *\*Paper Composition (Type & Weight for each layers) (e.g.: A160g/F120g/B120g):* | | | | |
| ***Paper Pallet-Feet:*** | *\*Feet Size: 180\*90mm, 140\*90mm,* *90\*90mm, 60\*90mm* | | | | |
|  | *\*Feet Filler Quality (e.g.:CB25):* | | *\*Feet Tray Quality(e.g.:CB10):* | | |
| ***Paper Pallet-Load Bearer****:*  *Description of* ***Corner mat for Penetration test:*** | *\*Load Bearer Code:* *LB05,* *LB10,*  *LB20, LB30 LB40, LB50* | | *\*Load Bearer Quality (e.g.:CB150/CB230):*  *Material Description:* | | |

**Additional Information**

**Date: Authorized signature & Company chop:**

***Test Item(s) Required (Please tick) and sample requirement:***

**Packaging general requirements, IOS-P-0010:**

Complete test **Corrugated board** (25pcs, 50\*50cm)

Flat crush test (FCT) ISO 3035 (3pcs, 50\*50cm)

Edgewise crush test (ECT) ISO 3037 (3pcs, 50\*50cm)

Thickness ISO 3034 (2pcs, 50\*50cm)

*Bursting strength test (BST) ISO 2759 (5pcs,* 50\*50cm)

Bending stiffness ISO 5628 (8pcs, 50\*50cm)

Cobb60 test ISO 535 (4pcs, 50\*50cm)

Nominal Weight (g/m2 ) (2pcs, 50\*50cm)

Flute type

Dry Weight (4pcs, 50\*50cm)

Mottling Coefficient (STFI Method) - only for white CB (3pcs, 20\*20cm) It is recommended to send of white top liners i.g. white papers for CBs

**Paper pallet**

Compression test for feet (15pcs feet)

Complete test **Load Bearer**

Load bearer sheet deflection test (10pcs on MD, 45\*10cm and 10pcs on CD direction, 45\*10cm)

Cobb60 test (15pcs, 14\*14cm)

Thickness

**Corner penetration test (15 pcs 10cm length)**

***Sample Submittal Guide****:1. The specimen should be provided with identification (e.g.: CB/LB/IF code) in one corner and be as small as practicable. 2. Each specimen shall be* ***kept flat, free from wrinkles and folds, and before converting process to boxes or pallets****.*